**ECE 233 Project Report**

**Hybrid Digital and Analog Beamforming Design**

**for Large-Scale Antenna Arrays**

**Ruoye Wang | 605625594**

**Yida Chen | 005852117**

**Abstract**

Abstract

TODO change figure number

**System Model**

This project implements a model proposed by the reference paper. This narrowband downlink single-cell multi-user MIMO system model has a two-stage hybrid digital and analog beamforming architecture at the base station (BS) and the user terminals. A picture containing diagram, plan, text, technical drawing

Description automatically generated

Figure : Block diagram of the model proposed by the paper

As the figure above shows, the BS has antennas and RF chains and serves users. Each user is equipped with antennas and RF chains and requires data streams. The number of data streams required by each user; the total number of data streams .

This project assumes single-user scenario, i.e., . To simplify the notation while preserving the generality, it is assumed that . The project first implements the hybrid beamformer design for the case where to show that, according to Proposition 1, a fully digital beamformer architecture can be realized by a hybrid structure with at least RF chains using a proposed heuristic algorithm. Then the same algorithm is implemented for the case where .

The symbols represent the digital precoder at the BS (size ), the RF precoder at the BS (size ), the digital combiner at the user end (size ), and the RF combiner at the user end (size ). (size ) is the matrix of the complex channel gains from the transmit antennas of the BS to the user (note that since , all can be represented by a single ; the same can be applied to other user-specific quantities in the paper).

Then, the transmitted signal can be represented by:

A picture containing font, text, white, typography

Description automatically generated

Where is the vector of data symbols. And the final processed signals are obtained as:

A picture containing font, text, handwriting, typography

Description automatically generated

Where represents the additive white Gaussian noise.

**Main Part**

This paper mainly focuses on maximizing the overall spectral efficiency with total transmit power constrained and fully known. This requires us to find the optimal solution for precoders at the transmitter end and the combiners at the receiver end, which can be represented by this formula:




Figure : the formula representing the main problem (K=1, disregarding k)

This formula is calculated under the aforementioned cases and . It can be simplified for precoder design:

A picture containing text, font, line, white

Description automatically generated

Figure : Precoder design formula

**scenario**

When , can be calculated by:




Figure : RF precoder design formula

Which is a simplification of Figure. 3 assuming . It is summarized in Algorithm 1:

A picture containing text, screenshot, font, number

Description automatically generated

Figure : Algorithm 1 to calculate RF precoder, with infinite resolution phase shifter

The formula to calculate is under the assumption of infinite phase shifters. Since accurate phase shifters can be expensive to implement in real world, they are commonly replaced by cost effective low resolution phase shifters. To simulate such phase shifters, the design of is quantized:

A picture containing text, font, white, diagram

Description automatically generated

Figure 6: RF precoder design, with 1-bit resolution phase shifter

Then can be calculated by solving:

A picture containing text, font, handwriting, line

Description automatically generated

Figure : Digital precoder design formula

Where and .

We use a water-filling solution (Reference: [Waterfilling](https://zhuanlan.zhihu.com/p/502453127)) to allocate power to each channel so that the overall channel capacity is maximized. The sum of power satisfies:

**A picture containing sketch, diagram, white, font

Description automatically generated**

Figure 8: Constraint on power allocation

Where the power of the first most efficient channels sum up to use to the largest extend. Since power cannot be negative:

A picture containing font, diagram, white, line

Description automatically generated

Figure 9: Formula to calculate allocated power


Combining the above two formulas, the water level chosen to satisfy the power sum constraints with equality can be represented by:

Figure 10: Formula to calculate water level

is obtained by iterating through the number of total channels . In each iteration, is calculated using the above formula, and compared with , where represents noise and is the square of right singular value of the SVD result of , since in Figure 6, the matrices are applied twice on both left and right. Similarly, the diagonal elements of are all square roots of . (Reference: Ruifu Donar Li)

The final value of is chosen so that satisfies the power constraint, as the following figure shows:

A picture containing diagram, line, technical drawing, rectangle

Description automatically generated

Figure : Water-filling solution

Then the matrix of digital precoder can be calculated using the formula proposed by the paper:

Where is the set of right singular vectors corresponding to the largest singular values of and is the diagonal matrix of allocated powers to each stream.

With designed, the formula in Figure 3 can be simplified to:

A picture containing text, font, line, white

Description automatically generated

Figure 12: RF combiner design formula

Due to its similarity to Figure 4, it can also be solved with Algorithm 1, with replaced by and since is large. The quantized is also calculated with the same method as .

Finally, the optimal digital combiner can be obtained from its MMSE solution:

A picture containing text, font, white, typography

Description automatically generated

Figure 13: Digital combiner design formula

After have been obtained, the performance of the model can be evaluated by its spectral efficiency:

A picture containing text, font, handwriting, white

Description automatically generated

Figure : Formula of spectral efficiency

The above process is repeated for a range of SNR, and for each SNR value, spectral efficiency is averaged over 100 Monte Carlo trials.

**scenario**


As stated in the paper, this scenario can still be implemented using the aforementioned process. It is implemented for .

**Results and Discussion**


1. A picture containing line, diagram, plot, parallel

   Description automatically generatedPlot the spectral efficiency vs. SNR in the range −10 dB to 6 dB, assuming a 64 × 16 MIMO system and .

The resulting figure is similar to Fig. 2 in the paper, with ~1.5dB difference on SNR values.

1. Plot the spectral efficiency vs. SNR in the range 0 dB to 30 dB, assuming a 10 × 10 MIMO system, , and phase shifters with 1-bit and infinite resolutions.

In paper Fig. 3, the spectral efficiency of 1-bit phase shifter is higher than that of infinite resolution phase shifter. However, this resulting figure shows the opposite. One possible reason is that, the paper’s beamformer is designed under the assumption of infinite resolution phase shifters and each entry of the RF beamformer is quantized to the nearest point of the set of possible phases. However, in this project, the beamformers for infinite resolution phase shifter is not quantized.


1. A picture containing line, plot, diagram

   Description automatically generatedPlot the spectral efficiency vs. SNR in the range −10 dB to 6 dB, assuming a 64 × 16 MIMO system, , and phase shifters with 1-bit and infinite resolutions.

The curves for 1-bit phase shifter are ~1.5dB lower than paper Fig. 4 which is considered acceptable error. Same as Fig. 4, the curves for infinite phase shifters (plotted separately for clarity) are significantly higher than that of 1-bit phase shifters, and the spectral efficiency increases as the number of RF chains increase, so that 1-bit phase shifter with more RF chains has a performance close to infinite phase shifters. This is in accordance with the paper’s conclusion that the number of RF chains can be used to trade off the accuracy of phase shifters in hybrid beamforming design.

A picture containing line, plot, diagram, text

Description automatically generatedThe above curves are rather unsmooth because the number of Monte Carlo trials are small. After the number of trials is increased to 1000, the figures become:



Which more clearly shows the paper’s discoveries.

**Conclusion**

Conclusion